/dts-v1/;

#include <tactility/bindings/root.h>
#include <tactility/bindings/esp32_ble.h>
#include <tactility/bindings/esp32_wifi_pinned.h>
#include <tactility/bindings/esp32_gpio.h>
#include <tactility/bindings/esp32_i2c.h>

/ {
	compatible = "root";
	model = "Heltec WiFi LoRa 32 V3";

	wifi0 {
		compatible = "espressif,esp32-wifi-pinned";
		status = "disabled";
	};

	ble0 {
		compatible = "espressif,esp32-ble";
		status = "disabled";
	};

	gpio0 {
		compatible = "espressif,esp32-gpio";
		gpio-count = <49>;
	};

	i2c_internal {
		compatible = "espressif,esp32-i2c";
		port = <I2C_NUM_0>;
		clock-frequency = <200000>;
		pin-sda = <&gpio0 17 GPIO_FLAG_NONE>;
		pin-scl = <&gpio0 18 GPIO_FLAG_NONE>;
	};
};
