/dts-v1/;

#include <tactility/bindings/root.h>
#include <tactility/bindings/battery_sense.h>
#include <tactility/bindings/esp32_adc_oneshot.h>
#include <tactility/bindings/esp32_ble.h>
#include <tactility/bindings/esp32_wifi_pinned.h>
#include <tactility/bindings/esp32_gpio.h>
#include <tactility/bindings/esp32_grove.h>
#include <tactility/bindings/esp32_i2c.h>
#include <tactility/bindings/esp32_i2s.h>
#include <tactility/bindings/esp32_spi.h>
#include <tactility/bindings/esp32_uart.h>
#include <bindings/bmi270.h>
#include <tactility/bindings/esp32_sdspi.h>
#include <tactility/bindings/esp32_pwm_ledc.h>
#include <tactility/bindings/pwm_backlight.h>

#include <bindings/st7789.h>
#include <bindings/cardputer_adv_keyboard.h>

// Reference: https://docs.m5stack.com/en/core/Cardputer-Adv
/ {
	compatible = "root";
	model = "M5Stack Cardputer Adv";

	wifi0 {
		compatible = "espressif,esp32-wifi-pinned";
		status = "disabled";
	};

	ble0 {
		compatible = "espressif,esp32-ble";
		status = "disabled";
	};

	gpio0 {
		compatible = "espressif,esp32-gpio";
		gpio-count = <49>;
	};

	adc0 {
		compatible = "espressif,esp32-adc-oneshot";
		unit-id = <ADC_UNIT_1>;
		clk-src = <ADC_RTC_CLK_SRC_DEFAULT>;
		// GPIO10 (ADC1_CHANNEL_9 on ESP32-S3): battery voltage sense, behind a 1:2 divider.
		channels = <ADC_CHANNEL_9 ADC_ATTEN_DB_12 ADC_BITWIDTH_DEFAULT>;
	};

	battery-sense {
		compatible = "battery-sense";
		io-channel = <&adc0 0>;
		reference-voltage-mv = <3300>;
		multiplier = <2000>;
	};

	i2c_internal {
		compatible = "espressif,esp32-i2c";
		port = <I2C_NUM_0>;
		clock-frequency = <400000>;
		pin-sda = <&gpio0 8 GPIO_FLAG_NONE>;
		pin-scl = <&gpio0 9 GPIO_FLAG_NONE>;

		bmi270 {
			compatible = "bosch,bmi270";
			reg = <0x69>;
		};

		keyboard {
			compatible = "m5stack,cardputer-adv-keyboard";
			reg = <0x34>;
		};
	};

	port_a: grove0 {
		compatible = "espressif,esp32-grove";
		defaultMode = <GROVE_MODE_I2C>;
		pinSdaTx = <&gpio0 2 GPIO_FLAG_NONE>;
		pinSclRx = <&gpio0 1 GPIO_FLAG_NONE>;
		uartPort = <UART_NUM_1>;
		i2cPort = <I2C_NUM_1>;
		i2cClockFrequency = <400000>;
	};

	display_backlight_pwm {
		compatible = "espressif,esp32-pwm-ledc";
		pin = <&gpio0 38 GPIO_FLAG_NONE>;
		period-ns = <1953125>;
		ledc-timer = <0>;
		ledc-channel = <0>;
	};

	display_backlight {
		compatible = "pwm-backlight";
		// Off by default so display power-on won't show the screen from before the last power loss.
		// The display backlight is turned on during the boot process.
		status = "disabled";
		pwm = <&display_backlight_pwm>;
	};

	spi0 {
		compatible = "espressif,esp32-spi";
		host = <SPI2_HOST>;
		cs-gpios = <&gpio0 37 GPIO_FLAG_NONE>;
		pin-mosi = <&gpio0 35 GPIO_FLAG_NONE>;
		pin-sclk = <&gpio0 36 GPIO_FLAG_NONE>;

		display@0 {
			compatible = "sitronix,st7789";
			horizontal-resolution = <240>;
			vertical-resolution = <135>;
			// Should be 52 according to https://github.com/m5stack/M5GFX/blob/master/src/M5GFX.cpp but this leaves a gap at the bottom
			gap-x = <53>;
			gap-y = <40>;
			swap-xy;
			mirror-x;
			invert-color;
			pixel-clock-hz = <62500000>;
			pin-dc = <&gpio0 34 GPIO_FLAG_NONE>;
			pin-reset = <&gpio0 33 GPIO_FLAG_NONE>;
			backlight = <&display_backlight>;
		};
	};

	spi1 {
		compatible = "espressif,esp32-spi";
		host = <SPI3_HOST>;
		cs-gpios = <&gpio0 12 GPIO_FLAG_NONE>,
		           <&gpio0 5 GPIO_FLAG_NONE>;
		pin-mosi = <&gpio0 14 GPIO_FLAG_NONE>;
		pin-miso = <&gpio0 39 GPIO_FLAG_NONE>;
		pin-sclk = <&gpio0 40 GPIO_FLAG_NONE>;
		miso-pull-up;

		sdcard@0 {
			compatible = "espressif,esp32-sdspi";
			status = "disabled";
			frequency-khz = <20000>;
		};
	};

	// Speaker and microphone (ES8311)
	i2s0 {
		compatible = "espressif,esp32-i2s";
		port = <I2S_NUM_0>;
		pin-bclk = <&gpio0 41 GPIO_FLAG_NONE>;
		pin-ws = <&gpio0 43 GPIO_FLAG_NONE>;
		pin-data-out = <&gpio0 42 GPIO_FLAG_NONE>;
		pin-data-in = <&gpio0 46 GPIO_FLAG_NONE>;
	};
};
