/dts-v1/;

#include <tactility/bindings/battery_sense.h>
#include <tactility/bindings/root.h>
#include <tactility/bindings/esp32_adc_oneshot.h>
#include <tactility/bindings/esp32_ble.h>
#include <tactility/bindings/esp32_gpio.h>
#include <tactility/bindings/esp32_grove.h>
#include <tactility/bindings/esp32_i2c.h>
#include <tactility/bindings/esp32_i2s.h>
#include <tactility/bindings/esp32_pwm_ledc.h>
#include <tactility/bindings/pwm_backlight.h>
#include <tactility/bindings/esp32_sdspi.h>
#include <tactility/bindings/esp32_spi.h>
#include <tactility/bindings/esp32_wifi_pinned.h>
#include <tactility/bindings/esp32_uart.h>
#include <tactility/bindings/esp32_usbdevice.h>

#include <bindings/gt911.h>
#include <bindings/st7789.h>
#include <bindings/es7210.h>
#include <bindings/dummy_i2s_amp.h>
#include <bindings/gpio_trackball.h>

#include <lilygo/bindings/tdeck_keyboard.h>
#include <lilygo/bindings/tdeck_keyboard_backlight.h>

// Reference: https://wiki.lilygo.cc/products/t-deck-series/t-deck/
/ {
	compatible = "root";
	model = "LilyGO T-Deck";

	adc0 {
		compatible = "espressif,esp32-adc-oneshot";
		unit-id = <ADC_UNIT_1>;
		clk-src = <ADC_RTC_CLK_SRC_DEFAULT>;
		channels = <ADC_CHANNEL_3 ADC_ATTEN_DB_12 ADC_BITWIDTH_DEFAULT>;
	};

	battery-sense {
		compatible = "battery-sense";
		io-channel = <&adc0 0>;
		reference-voltage-mv = <3300>;
		multiplier = <2110>;
	};

	wifi0 {
		compatible = "espressif,esp32-wifi-pinned";
		status = "disabled";
	};

	ble0 {
		compatible = "espressif,esp32-ble";
		status = "disabled";
	};

	gpio0 {
		compatible = "espressif,esp32-gpio";
		gpio-count = <49>;
	};

	trackball {
		compatible = "tactility,gpio-trackball";
		pin-right = <&gpio0 2 GPIO_FLAG_NONE>;
		pin-up = <&gpio0 3 GPIO_FLAG_NONE>;
		pin-left = <&gpio0 1 GPIO_FLAG_NONE>;
		pin-down = <&gpio0 15 GPIO_FLAG_NONE>;
		pin-click = <&gpio0 0 GPIO_FLAG_NONE>;
	};

	// i2s0 and i2s1 are declared before i2c0 so i2s1 has started before the es7210 codec (below) references it.
	// Speaker I2S (MAX98357A amplifier)
	i2s0 {
		compatible = "espressif,esp32-i2s";
		port = <I2S_NUM_0>;
		pin-bclk = <&gpio0 7 GPIO_FLAG_NONE>;
		pin-ws = <&gpio0 5 GPIO_FLAG_NONE>;
		pin-data-out = <&gpio0 6 GPIO_FLAG_NONE>;
	};

	// Microphone I2S (ES7210), separate port from the speaker
	i2s1 {
		compatible = "espressif,esp32-i2s";
		port = <I2S_NUM_1>;
		pin-bclk = <&gpio0 47 GPIO_FLAG_NONE>;
		pin-ws = <&gpio0 21 GPIO_FLAG_NONE>;
		pin-data-in = <&gpio0 14 GPIO_FLAG_NONE>;
		pin-mclk = <&gpio0 48 GPIO_FLAG_NONE>;
	};

	// MAX98357A class-D speaker amplifier. No I2C. Per schematic, SD_MODE/GAIN_SLOT is
	// tied via fixed resistors (R21/R22), not driven by an MCU GPIO -- the amp is always
	// enabled when powered, so no enable-gpio is wired here.
	speaker0 {
		compatible = "maxim,max98357a";
		i2s = <&i2s0>;
	};

	i2c_internal: i2c0 {
		compatible = "espressif,esp32-i2c";
		port = <I2C_NUM_0>;
		clock-frequency = <100000>;
		pin-sda = <&gpio0 18 GPIO_FLAG_NONE>;
		pin-scl = <&gpio0 8 GPIO_FLAG_NONE>;

		// WARNING: Don't use the interrupt pin as it's unstable on some devices
		touch {
			compatible = "goodix,gt911";
			reg = <0x5D>;
			x-max = <240>;
			y-max = <320>;
			swap-xy;
			mirror-x;
		};

		keyboard {
			compatible = "lilygo,tdeck-keyboard";
			reg = <0x55>;
		};

		keyboard_backlight {
			compatible = "lilygo,tdeck-keyboard-backlight";
			reg = <0x55>;
		};

		// ES7210 microphone ADC. Per schematic all 4 MSM381A3729H9CP mic capsules are
		// populated (MIC1-4), and AD0/AD1 are unconnected (default low -> address 0x40).
		// Stock LilyGO firmware drives MIC1/MIC2 at 0dB and MIC3/MIC4 at 37.5dB gain --
		// the es7210 driver here applies a single gain to all active mics, so per-pair
		// gain differentiation is not yet replicated.
		es7210 {
			compatible = "everest,es7210";
			reg = <0x40>;
			i2s = <&i2s1>;
			mic-mask = <15>;
		};
	};

	display_backlight_pwm {
		compatible = "espressif,esp32-pwm-ledc";
		pin = <&gpio0 42 GPIO_FLAG_NONE>;
		// 32 KHz and higher causes the screen to start dimming again above 80% brightness
		// when moving the brightness slider rapidly from a lower setting to 100% (debug-traced, not a slider bug).
		period-ns = <33333>;
		ledc-timer = <0>;
		ledc-channel = <0>;
	};

	display_backlight {
		compatible = "pwm-backlight";
		// Off by default so dispaly power-on won't show the screen from before the last power loss.
		// The display backlight is turned on during the boot process.
		status = "disabled";
		pwm = <&display_backlight_pwm>;
	};

	spi0 {
		compatible = "espressif,esp32-spi";
		host = <SPI2_HOST>;
		cs-gpios = <&gpio0 12 GPIO_FLAG_NONE>, // Display
		            <&gpio0 39 GPIO_FLAG_NONE>, // SD card
					<&gpio0 9 GPIO_FLAG_NONE>;  // Radio
		pin-mosi = <&gpio0 41 GPIO_FLAG_NONE>;
		pin-miso = <&gpio0 38 GPIO_FLAG_NONE>;
		pin-sclk = <&gpio0 40 GPIO_FLAG_NONE>;

		display@0 {
			compatible = "sitronix,st7789";
			horizontal-resolution = <320>;
			vertical-resolution = <240>;
			swap-xy;
			mirror-x;
			invert-color;
			pixel-clock-hz = <62500000>;
			pin-dc = <&gpio0 11 GPIO_FLAG_NONE>;
			backlight = <&display_backlight>;
		};

		// Must be started after display
		sdcard@1 {
			compatible = "espressif,esp32-sdspi";
			status = "disabled";
			frequency-khz = <20000>;
		};
	};

	grove0 {
		compatible = "espressif,esp32-grove";
		defaultMode = <GROVE_MODE_I2C>;
		pinSdaTx = <&gpio0 43 GPIO_FLAG_NONE>;
		pinSclRx = <&gpio0 44 GPIO_FLAG_NONE>;
		uartPort = <UART_NUM_1>;
		i2cPort = <I2C_NUM_1>;
		i2cClockFrequency = <400000>;
	};

	usbdevice0 {
		compatible = "espressif,esp32-usbdevice";

		usbdevicemsc0 {
			compatible = "espressif,esp32-usbdevice-msc";
		};
	};
};
